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[bookmark: _Toc226628448][bookmark: _Toc227158421][bookmark: _Toc227158892]When to Use This Form - This paper Safety Permit is for temporary use only when Beakon is unavailable due to a system outage, a communication black spot, or another issue that prevents the system from being used.
When Not to Use This Form - Do not use this form if Beakon is available. This includes situations where a person is waiting for an account, has forgotten their login details, does not have a device available, or is experiencing delays in obtaining access.
What to Do Once Access Is Restored - As soon as access to Beakon is restored, the permit must be created in Beakon. A copy of the completed paper permit must be uploaded and attached to the electronic permit record.
	Permit Applicant information (This section is mandatory)

	Name
	

	Organisation
	

	Email
	
	Mobile
	

	Permit Holder information (This section is mandatory)

	Name
	

	Organisation
	

	Email
	
	Mobile
	

	Safety Permit Information (This section is mandatory)

	Unitywater representative
	
	
	

	Worksite address
	
	
	

	Description of work
	
	
	

	Work order #
	

	Safety Permit type
	☐ Confined space entry
	☐ Excavation
	☐ High voltage electrical

	
	☐ Hot work
	☐ Lifting
	☐ Work at height

	Permit start date
	
	Time
	

	Expected work duration
	

	Permit end date
	
	Time
	

	Comments
	

	Related Safety Permits
(if applicable)
	

	Risk Assessment 
Must be completed before permit is approved
	Unitywater team members: use F10656 – Risk Assessment Template
Contractors: use own Risk Assessment template or contact UW Representative for copy of F10656 – Risk Assessment Template. 

	Work Group
(list name of everyone involved in the work)
	

	As the permit holder, I confirm all work group members have been made aware of all identified risks and controls. 
	
	

	
	Permit Holder Signature
	Date




	Confined space atmospheric testing log (This section is mandatory before entering a confined space)

	Person conducting atmospheric testing
	

	Standby Person
	

	Hydrogen sulphide H2S
(safe range <10ppm)
	
	Oxygen O2
(safe range 19.5% - 23.5%)
	

	Carbon monoxide CO
(safe range <30ppm)
	
	Flammable Gases LELs
(safe range <10% of LEL)
	

	Comments/ additional gas types tested
	

	Safety Permit Questions (This section is mandatory for the relevant Safety Permit Types selected. You must not commence work if you answer NO to any of the relevant questions.)

	Confined Space Entry Safety Permit 

	Is everyone involved in the confined space entry trained an competent for their role?
	☐ Yes   ☐ No

	Have all energy sources, services and engulfment hazards been isolated and made safe before entry? 
	☐ Yes   ☐ No

	Has the atmosphere been tested, is it safe to enter, and will it continue to be monitored while work is underway?
	☐ Yes   ☐ No

	Is a rescue plan in place, does everyone understand it, and are trained rescue people and equipment immediately available? 
	☐ Yes   ☐ No

	Are controls in place to stop people entering the confined space who shouldn’t be there? 
	☐ Yes   ☐ No

	Is a Standby Person in place and able to maintain communication with entrants throughout the work? 
	☐ Yes   ☐ No

	[image: Warning with solid fill]If you answered NO to any of the questions above, you must not start confined space entry. 

	Excavation Safety Permit 

	Has BYDA (Before You Dig Australia) been checked and do you know how you’ll safely uncover any services before digging? 
	☐ Yes   ☐ No

	Will the excavation be benched, battered, shored or otherwise protected from collapse?
	☐ Yes   ☐ No

	Will the excavation be protected to stop people entering or falling into it?
	☐ Yes   ☐ No

	Is there a safe way for people to enter and exit the excavation?
	☐ Yes   ☐ No

	Could water enter or flood the excavation and, if so, are controls in place? 
	☐ Yes   ☐ No

	[image: Warning with solid fill]If you answered NO to any of the questions above, you must not start excavation work. 




	Safety Permit Questions (This section is mandatory for the relevant Safety Permit Types selected. You must not commence work if you answer NO to any of the relevant questions.)

	High voltage electrical Safety Permit 

	Has written consent been obtained from Unitywater’s High Voltage Responsible Person for this high voltage work?
	☒ Yes   ☐ No

	Are all people involved trained, competent and authorised to perform this high voltage electrical work? 
	☐ Yes   ☐ No

	Have all energy sources been identified and isolated (LOTO)?
	☐ Yes   ☐ No

	Are appropriate access restrictions, warning systems and exclusion measures in place and understood?
	☐ Yes   ☐ No

	Have arc flash risks been assessed, and is the required PPE being used?
	☐ Yes   ☐ No

	[image: Warning with solid fill]If you answered NO to any of the questions above, you must not start high voltage electrical work. 

	Hot work Safety Permit 

	Have combustible materials been removed or protected to prevent fire?
	☐ Yes   ☐ No

	Has a Fire Watch been appointed and is firefighting equipment ready to use?
	☐ Yes   ☐ No

	Have the current fire danger rating and any fire restrictions been checked on the Queensland Fire Department (QFD) website, and have any required approvals been obtained?
	☐ Yes   ☐ No

	Has the atmosphere been tested and confirmed safe for hot work where required?
	☐ Yes   ☐ No

	Have all energy sources been identified and isolated (LOTO)?
	☐ Yes   ☐ No

	[image: Warning with solid fill]If you answered NO to any of the questions above, you must not start hot work. 

	Lifting Safety Permit 

	Is everyone involved in the lift trained, competent and licensed for their role where required?
	☐ Yes   ☐ No

	Has the lift location been checked and can the ground safely support the lifting equipment? 
	☐ Yes   ☐ No

	Is a Lift Plan in place and has it been communicated to everyone involved in the lift?
	☐ Yes   ☐ No

	Are controls in place to keep people away from the lifting area?
	☐ Yes   ☐ No

	Has all lifting equipment and lifting gear been inspected and confirmed safe to use?
	☐ Yes   ☐ No

	Are controls in place to keep the load under control and prevent line-of-fire risks?
	☐ Yes   ☐ No

	[image: Warning with solid fill]If you answered NO to any of the questions above, you must not start lifting activities. 

	Working at heights Safety Permit 

	Is everyone involved in the work at height trained and competent for their role?
	☐ Yes   ☐ No

	Are suitable controls in place to prevent a fall?
	☐ Yes   ☐ No

	Are controls in place to prevent objects falling onto people, plant or assets below?
	☐ Yes   ☐ No

	Is a rescue plan in place, does everyone understand it, and are trained rescue people and equipment immediately available?
	☐ Yes   ☐ No

	[image: Warning with solid fill]If you answered NO to any of the questions above, you must not start working at heights. 

	Confined space entry and exit record (This section is mandatory if entering a confined space. If more records are required, please attach) 

	[bookmark: _Hlk240292651]Person 1

	First and last name
	

	Time in
	
	Time out
	

	Person 2

	First and last name
	

	Time in
	
	Time out
	

	Person 3

	First and last name
	

	Time in
	
	Time out
	

	Person 4

	First and last name
	

	Time in
	
	Time out
	

	Hot work log (This section is mandatory if undertaking hot work. If more records are required, please attach) 

	Hot work activity 1

	Start time
	
	End time
	

	Hot work activity 2

	Start time
	
	End time
	

	Fire Watch (30 minutes after hot work stops)

	Start time
	
	End time
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